flush count: 1
pts seen nr: 15
pts seen: 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14
nonfail test: ok
recovery test: ok
flush count: 1
pts seen nr: 15
pts seen: 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14
overflow without packet dropping: ok
overflow with packet dropping: ok
